Hello, here we have a resistor and inductor together “RL”, with a capacitor in parallel.

We have an AC source, ammeter measuring the supply current and then we understand with a junction the current gets split because it is a flow, so the sum of currents is the same as the supply.

Hope this helps.

Thank you for listening.